{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["废气排放","废水排放"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气排放","index":0,"n_rows":45,"n_cols":24,"rows_kept":45,"merged":[[1,0,44,0],[5,1,7,1],[9,1,28,1],[32,1,44,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/h)","温度(°C)","湿度(%)","含氧量(%)","流速(m/s)","生产负荷(%)","实测浓度","折算浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["011","江苏海云花新材料有限公司","水环境,大气环境,土壤污染监管","化学试剂和助剂制造","化学工业挥发性有机物排放标准（江苏省地方标准）(DB32/3151-2016)","表1","甲类车间DA001排气筒","非甲烷总烃","2025-11-13","3877","19","3.2","","6","","0.54","0.54","80","","mg/m3","否","","","是"]
["011","宜兴中车时代半导体有限公司","水环境,大气环境,环境风险管控","半导体分立器件制造","半导体行业污染物排放标准(DB 32/3747-2020)","表3大气污染物排放限值","芯片车间DA006排气筒","非甲烷总烃","2025-11-20","67462","15","1.48","","9.8","","0.70","0.70","50","","mg/m3","否","","","是"]
["011","宜兴市炜华合金材料有限公司","大气环境","有色金属合金制造","江苏省大气综合排放标准(DB32/4041-2021)","表1 大气污染物有组织排放限值","混合废气排气筒DA002(001)","非甲烷总烃","2025-11-21","392","28","1.81","","1.7","","0.12","0.12","60","","mg/m3","否","","","是"]
["011","江苏雷蒙新材料有限公司","水环境,地下水,大气环境,土壤污染监管,环境风险管控","化学试剂和助剂制造","化学工业挥发性有机物排放标准(DB  32/3151—2016)","表1 挥发性有机物及臭气浓度排放限值","GTA废气排放DA003","非甲烷总烃","2025-11-12","73","17","3.08","","0.7","","0.13","0.13","80","","mg/m3","否","","","是"]
["011","宜兴市苏南固废处理有限公司","大气环境,土壤污染监管,环境风险管控","危险废物治理","江苏省地方标准大气污染物综合排放标准(DB32/4041-2021)","表1 大气污染物有组织排放限值,其他","车间排放口","汞及其化合物","2025-08-14","1023","","2.4","","10.6","","<0.0025","<0.0025","0.01","","mg/m3","否","","","是"]
["011","宜兴市苏南固废处理有限公司","大气环境,土壤污染监管,环境风险管控","危险废物治理","《江苏省大气污染物综合排放标准》(DB32/4041-2021)","表 1 大气污染物有组织排放限值,其他,最高允许排放浓度","车间排放口","颗粒物","2025-08-14","1023","","2.4","","10.6","","9.0","9.0","20","","mg/m3","否","","","是"]
["011","宜兴市苏南固废处理有限公司","大气环境,土壤污染监管,环境风险管控","危险废物治理","《江苏省大气污染物综合排放标准》(DB32/4041-2021)","表 1 大气污染物有组织排放限值,其他,最高允许排放浓度","车间排放口","氮氧化物","2025-08-14","1050","","2.4","20.7","10.9","","<3","<3","100","","mg/m3","否","","","是"]
["011","江苏金道生物科技有限公司","大气环境,土壤污染监管,环境风险管控","复混肥料制造","江苏省地方标准大气污染物综合排放标准(DB32/4041-2021)","表1 大气污染物有组织排放限值,其他","DA003","氟化物","2025-09-23","10832","60","9.2","","3.1","","0.27","0.27","3","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","3线排气筒","颗粒物","2025-08-15","124538","173.5","23.8","9","14.1","","1.9","1.5","30","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","3线排气筒","镉、铊及其化合物（以Cd +Tl计）","2025-08-15","118144","173.1","24.4","8.6","13.4","","0.0000396","0.0000318","0.1","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","3线排气筒","锑，砷，铅，铬，钴，铜，锰，镍及其化合物（以Sb+As+Pb+Cr+Co+Cu+Mn+Ni计）","2025-08-15","118144","173.1","24.4","8.6","13.4","","0.0397","0.0318","1.0","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","3线排气筒","二氧化硫","2025-08-15","124538","173.5","23.8","9","14.1","","4","3","100","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","3线排气筒","汞及其化合物","2025-08-15","118144","","","","","","<0.0025","<0.0025","0.05","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表2）新建生活垃圾焚烧排放烟气中一氧化碳浓度限值,1小时均值","3线排气筒","一氧化碳","2025-08-15","124538","173.5","23.8","9","14.1","","<3","<3","100","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","3线排气筒","氯化氢","2025-08-15","124538","173.5","23.8","9","14.1","","4.80","3.97","60","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","3线排气筒","二噁英类","2025-06-30","","","","","","","0.014","0.014","0.1","","ng-TEQ/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","3线排气筒","二噁英类","2025-08-15","","","","","","","0.017","0.017","0.1","","ng-TEQ/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","3线排气筒","氮氧化物","2025-08-15","124538","173.5","23.8","9","14.1","","104","85","300","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","4线排气筒","二噁英类","2025-06-30","","","","","","","0.0095","0.0095","0.1","","ng-TEQ/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","4线排气筒","二氧化硫","2025-08-15","126052","176.2","26.7","9.2","14.9","","6","5","100","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表2）新建生活垃圾焚烧排放烟气中一氧化碳浓度限值,1小时均值","4线排气筒","一氧化碳","2025-08-15","126052","176.2","26.7","9.2","","","<3","<3","100","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","4线排气筒","二噁英类","2025-08-15","","","","","","","0.0072","0.0072","0.1","","ng-TEQ/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","4线排气筒","氮氧化物","2025-08-15","126052","176.2","26.7","9.2","14.9","","108","92","300","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","4线排气筒","颗粒物","2025-08-15","124064","175.5","26.1","9.7","14.5","","2.1","1.9","30","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","4线排气筒","锑，砷，铅，铬，钴，铜，锰，镍及其化合物（以Sb+As+Pb+Cr+Co+Cu+Mn+Ni计）","2025-08-15","120901","174.7","25.3","10","14","","0.0691","0.0626","1.0","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","4线排气筒","镉、铊及其化合物（以Cd +Tl计）","2025-08-15","120901","174.7","25.3","10","14","","0.0000913","0.0000826","0.1","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,1小时均值","4线排气筒","氯化氢","2025-08-15","126052","176.2","26.7","9.2","14.9","","1.03","0.87","60","","mg/m3","否","","","是"]
["011","光大环保能源（宜兴）有限公司","水环境,大气环境,土壤污染监管,环境风险管控","生物质能发电-生活垃圾焚烧发电","生活垃圾焚烧污染控制标准(GB18485-2014)","（表4）生活垃圾焚烧排放烟气中污染物限值,测定均值","4线排气筒","汞及其化合物","2025-08-15","120901","174.7","25.3","10","14","","<0.0025","<0.0025","0.05","","mg/m3","否","","","是"]
["011","宜兴市博辉特种纤维有限公司","大气环境","涤纶纤维制造","江苏省大气综合排放标准(DB32/4041-2021)","表1 大气污染物有组织排放限值","POY纺丝车间废气排气筒","非甲烷总烃","2025-11-13","1312","19","2.51","","5.6","","0.96","0.96","60","","mg/m3","否","","","是"]
["011","江苏格桑花涂料有限公司","水环境,地下水,大气环境,土壤污染监管","涂料制造","涂料、油墨及胶粘剂工业大气污染物排放标准(GB37824—2019)","（表2）大气污染物特别排放限值,车间或生产设施排气筒,涂料制造、油墨及类似产品制造","生产车间DA011工艺废气排放口","非甲烷总烃","2025-11-11","9077","18","1.84","","5.4","","43.5","43.5","60","","mg/m3","否","","","是"]
["011","江苏华宜针织有限公司","水环境,大气环境","棉印染精加工","江苏省大气综合排放标准(DB32/4041-2021)","表1 大气污染物有组织排放限值","定型机车间","非甲烷总烃","2025-11-12","","","","","","","0.14","0.14","60","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB18484-2001)","（表3）危险废物焚烧炉大气污染物排放限值,不同焚烧容量时的最高允许排放浓度限值（mg/m3）","焚烧炉排气筒(DA001)","铬、锡、锑、铜、锰及其化合物","2025-08-13","31736","77.7","","13.1","8.3","","0.0459","0.0576","2","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB18484-2001)","（表3）危险废物焚烧炉大气污染物排放限值,不同焚烧容量时的最高允许排放浓度限值（mg/m3）","焚烧炉排气筒(DA001)","砷、镍及其化合物","2025-08-13","31736","77.7","","13.1","8.3","","0.0246","0.0308","0.5","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","焚烧炉排气筒(DA001)","颗粒物","2025-08-13","31736","77.7","","13.1","8.3","","2.3","2.6","30","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","焚烧炉排气筒(DA001)","氯化氢","2025-08-13","31736","77.7","","13.1","8.3","","1.26","1.51","60","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","焚烧炉排气筒(DA001)","氮氧化物","2025-08-13","31736","77.7","","13.1","8.3","","60","72","300","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","焚烧炉排气筒(DA001)","二氧化硫","2025-08-13","31736","77.7","","13.1","8.3","","6","7","100","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","焚烧炉排气筒(DA001)","氟化氢","2025-08-13","31736","77.7","","13.1","8.3","","<0.08","<0.08","4","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB18484-2001)","（表3）危险废物焚烧炉大气污染物排放限值,不同焚烧容量时的最高允许排放浓度限值（mg/m3）","焚烧炉排气筒(DA001)","二噁英类","2025-06-27","","","","","","","0.017","0.017","0.5","","TEQ ng/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,1 小时均值","焚烧炉排气筒(DA001)","一氧化碳","2025-08-13","31736","77.7","","13.1","8.3","","3","4","100","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","焚烧炉排气筒(DA001)","汞及其化合物","2025-08-13","31736","77.7","","13.1","8.3","","<0.0025","<0.0025","0.05","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","焚烧炉排气筒(DA001)","铅及其化合物","2025-08-13","31736","77.7","","13.1","8.3","","0.00503","0.00641","0.5","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","焚烧炉排气筒(DA001)","镉及其化合物","2025-08-13","31736","77.7","","13.1","8.3","","0.000164","0.000205","0.05","","mg/m3","否","","","是"]
["011","宜兴市凌霞固废处置有限公司","水环境,大气环境,土壤污染监管,环境风险管控","危险废物治理-焚烧","危险废物焚烧污染控制标准(GB 18484—2020)","表 3 危险废物焚烧设施烟气污染物排放浓度限值,测定均值","焚烧炉排气筒(DA001)","二噁英类","2025-08-13","","","","","","","0.027","0.027","0.5","","ng TEQ/Nm3","否","","","是"]

{"sheet":"废水排放","index":1,"n_rows":43,"n_cols":22,"rows_kept":43,"merged":[[1,0,42,0],[1,1,4,1],[5,1,9,1],[10,1,13,1],[14,1,17,1],[18,1,21,1],[22,1,27,1],[28,1,32,1],[33,1,36,1],[37,1,42,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["011","江苏海云花新材料有限公司","水环境,大气环境,土壤污染监管","化学试剂和助剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","待排池(DW002)","化学需氧量","2025-11-13","","","","","258","500","","mg/L","否","","","是"]
["011","江苏海云花新材料有限公司","水环境,大气环境,土壤污染监管","化学试剂和助剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","待排池(DW002)","总氮（以N计）","2025-11-13","","","","","11.0","70","","mg/L","否","","","是"]
["011","江苏海云花新材料有限公司","水环境,大气环境,土壤污染监管","化学试剂和助剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","待排池(DW002)","氨氮（NH3-N）","2025-11-13","","","","","5.05","45","","mg/L","否","","","是"]
["011","江苏海云花新材料有限公司","水环境,大气环境,土壤污染监管","化学试剂和助剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","待排池(DW002)","总磷（以P计）","2025-11-13","","","","","1.53","8","","mg/L","否","","","是"]
["011","宜兴中车时代半导体有限公司","水环境,大气环境,环境风险管控","半导体分立器件制造","","半导体行业污染物排放标准江苏(DB32/3747-2020)","水污染物","工业废水排放口1(DW001)","化学需氧量","2025-11-20","","","","","24","300","","mg/L","否","","","是"]
["011","宜兴中车时代半导体有限公司","水环境,大气环境,环境风险管控","半导体分立器件制造","","半导体行业污染物排放标准江苏(DB32/3747-2020)","水污染物","工业废水排放口1(DW001)","氨氮（NH3-N）","2025-11-20","","","","","4.89","20","","mg/L","否","","","是"]
["011","宜兴中车时代半导体有限公司","水环境,大气环境,环境风险管控","半导体分立器件制造","","半导体行业污染物排放标准江苏(DB32/3747-2020)","水污染物","工业废水排放口1(DW001)","氟化物","2025-11-20","","","","","1.58","15","","mg/L","否","","","是"]
["011","宜兴中车时代半导体有限公司","水环境,大气环境,环境风险管控","半导体分立器件制造","","半导体行业污染物排放标准江苏(DB32/3747-2020)","水污染物","工业废水排放口1(DW001)","总氮（以N计）","2025-11-20","","","","","9.91","35","","mg/L","否","","","是"]
["011","宜兴中车时代半导体有限公司","水环境,大气环境,环境风险管控","半导体分立器件制造","","半导体行业污染物排放标准江苏(DB32/3747-2020)","水污染物","工业废水排放口1(DW001)","总磷（以P计）","2025-11-20","","","","","0.26","3","","mg/L","否","","","是"]
["011","江苏鹏鹞药业有限公司","水环境","化学药品制剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","接管口(DW001)","总磷（以P计）","2025-11-20","","","","","0.80","8","","mg/L","否","","","是"]
["011","江苏鹏鹞药业有限公司","水环境","化学药品制剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","接管口(DW001)","氨氮（NH3-N）","2025-11-20","","","","","6.60","45","","mg/L","否","","","是"]
["011","江苏鹏鹞药业有限公司","水环境","化学药品制剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","接管口(DW001)","总氮（以N计）","2025-11-20","","","","","16.1","70","","mg/L","否","","","是"]
["011","江苏鹏鹞药业有限公司","水环境","化学药品制剂制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","接管口(DW001)","化学需氧量","2025-11-20","","","","","25","500","","mg/L","否","","","是"]
["011","江苏雷蒙新材料有限公司","水环境,地下水,大气环境,土壤污染监管,环境风险管控","化学试剂和助剂制造","","化学工业水污染物排放标准（地标）(DB32/939-2020)","化学原料及化学制品制造业表一限值","接管处(001)","化学需氧量","2025-11-12","","","","","18","70","","mg/L","否","","","是"]
["011","江苏雷蒙新材料有限公司","水环境,地下水,大气环境,土壤污染监管,环境风险管控","化学试剂和助剂制造","","化学工业水污染物排放标准(DB 32/939-2020)","企业主要水污染物排放限值","接管处(001)","氨氮（NH3-N）","2025-11-12","","","","","0.68","8","","mg/L","否","","","是"]
["011","江苏雷蒙新材料有限公司","水环境,地下水,大气环境,土壤污染监管,环境风险管控","化学试剂和助剂制造","","化学工业水污染物排放标准（地标）(DB32/939-2020)","化学原料及化学制品制造业表一限值","接管处(001)","总磷（以P计）","2025-11-12","","","","","<0.01","0.5","","mg/L","否","","","是"]
["011","江苏雷蒙新材料有限公司","水环境,地下水,大气环境,土壤污染监管,环境风险管控","化学试剂和助剂制造","","化学工业水污染物排放标准（地标）(DB32/939-2020)","化学原料及化学制品制造业表一限值","接管处(001)","总氮（以N计）","2025-11-12","","","","","2.14","20","","mg/L","否","","","是"]
["011","宜兴市建东环保材料有限公司","水环境,土壤污染监管","无机盐制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","接管处","总氮（以N计）","2025-11-21","","","","","10.2","70","","mg/L","否","","","是"]
["011","宜兴市建东环保材料有限公司","水环境,土壤污染监管","无机盐制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","接管处","氨氮（NH3-N）","2025-11-21","","","","","4.79","45","","mg/L","否","","","是"]
["011","宜兴市建东环保材料有限公司","水环境,土壤污染监管","无机盐制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","接管处","总磷（以P计）","2025-11-21","","","","","1.24","8","","mg/L","否","","","是"]
["011","宜兴市建东环保材料有限公司","水环境,土壤污染监管","无机盐制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","接管处","化学需氧量","2025-11-21","","","","","125","500","","mg/L","否","","","是"]
["011","江苏驰马科技股份有限公司","水环境","日用杂品制造","","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,非蜡染行业间接排放","接管处","总氮（以N计）","2025-11-11","","","","","13.2","30","","mg/L","否","","","是"]
["011","江苏驰马科技股份有限公司","水环境","日用杂品制造","","纺织染整工业废水中锑污染物排放标准(DB32/3432-2018)","表1 纺织染整企业废水中总锑排放限值,太湖地区,间接排放,废水进入污水处理厂","接管处","总锑","2025-11-11","","","","","0.00830","0.08","","mg/L","否","","","是"]
["011","江苏驰马科技股份有限公司","水环境","日用杂品制造","","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","接管处","总磷（以P计）","2025-11-11","","","","","0.63","1.5","","mg/L","否","","","是"]
["011","江苏驰马科技股份有限公司","水环境","日用杂品制造","","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,通用","接管处","pH值","2025-11-11","","","","","7.45","9","6","无量纲","否","","","是"]
["011","江苏驰马科技股份有限公司","水环境","日用杂品制造","","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放,蜡染行业直接排放","接管处","氨氮（NH3-N）","2025-11-11","","","","","0.12","20","","mg/L","否","","","是"]
["011","江苏驰马科技股份有限公司","水环境","日用杂品制造","","纺织染整工业水污染物排放标准(GB4287-2012)","（表1）现有企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放,其他","接管处","化学需氧量","2025-11-11","","","","","22","200","","mg/L","否","","","是"]
["011","宜兴市舜昌亚麻纺织有限公司","水环境","麻纤维纺前加工和纺纱","","麻纺工业水污染物排放标准(GB28938-2012)","（表1、表2）现有和新建企业水污染物排浓度放限值及单位产品基准排水量,企业废水总排放口,间接排放","接管处","总磷（以P计）","2025-11-21","","","","","0.63","1.5","","mg/L","否","","","是"]
["011","宜兴市舜昌亚麻纺织有限公司","水环境","麻纤维纺前加工和纺纱","","纺织染整工业废水中锑污染物排放标准(DB32/3432-2018)","表1 纺织染整企业废水中总锑排放限值,太湖地区,间接排放,废水进入污水处理厂","接管处","总锑","2025-11-21","","","","","<0.0002","0.08","","mg/L","否","","","是"]
["011","宜兴市舜昌亚麻纺织有限公司","水环境","麻纤维纺前加工和纺纱","","麻纺工业水污染物排放标准(GB28938-2012)","（表1、表2）现有和新建企业水污染物排浓度放限值及单位产品基准排水量,企业废水总排放口,间接排放","接管处","总氮（以N计）","2025-11-21","","","","","25.7","30","","mg/L","否","","","是"]
["011","宜兴市舜昌亚麻纺织有限公司","水环境","麻纤维纺前加工和纺纱","","麻纺工业水污染物排放标准(GB28938-2012)","（表1、表2）现有和新建企业水污染物排浓度放限值及单位产品基准排水量,企业废水总排放口,间接排放","接管处","化学需氧量","2025-11-21","","","","","233","250","","mg/L","否","","","是"]
["011","宜兴市舜昌亚麻纺织有限公司","水环境","麻纤维纺前加工和纺纱","","麻纺工业水污染物排放标准(GB28938-2012)","（表1、表2）现有和新建企业水污染物排浓度放限值及单位产品基准排水量,企业废水总排放口,间接排放","接管处","氨氮（NH3-N）","2025-11-21","","","","","20.3","25","","mg/L","否","","","是"]
["011","江苏格桑花涂料有限公司","水环境,地下水,大气环境,土壤污染监管","涂料制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","污水排放口(DW001)","氨氮（NH3-N）","2025-11-11","","","","","2.80","45","","mg/L","否","","","是"]
["011","江苏格桑花涂料有限公司","水环境,地下水,大气环境,土壤污染监管","涂料制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","污水排放口(DW001)","总磷（以P计）","2025-11-11","","","","","0.21","8","","mg/L","否","","","是"]
["011","江苏格桑花涂料有限公司","水环境,地下水,大气环境,土壤污染监管","涂料制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","污水排放口(DW001)","化学需氧量","2025-11-11","","","","","16","500","","mg/L","否","","","是"]
["011","江苏格桑花涂料有限公司","水环境,地下水,大气环境,土壤污染监管","涂料制造","","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水排放口(DW001)","总氮（以N计）","2025-11-11","","","","","2.90","45","","mg/L","否","","","是"]
["011","江苏华宜针织有限公司","水环境,大气环境","棉印染精加工","","纺织染整工业废水中锑污染物排放标准[地标](DB32/3432-2018)","表1 纺织染整企业废水中总锑排放限值,太湖地区直接排放","接管处(DW002)","总锑","2025-11-12","","","","","0.00112","0.08","","mg/L","否","","","是"]
["011","江苏华宜针织有限公司","水环境,大气环境","棉印染精加工","","纺织染整工业水污染物排放标准(GB4287-2012)","表2新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口","接管处(DW002)","氨氮（NH3-N）","2025-11-12","","","","","9.72","20","","mg/L","否","","","是"]
["011","江苏华宜针织有限公司","水环境,大气环境","棉印染精加工","","纺织染整工业水污染物排放标准(GB4287-2012)","表2新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口","接管处(DW002)","总氮（以N计）","2025-11-12","","","","","9.88","30","","mg/L","否","","","是"]
["011","江苏华宜针织有限公司","水环境,大气环境","棉印染精加工","","纺织染整工业水污染物排放标准(GB4287-2012)","表2新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口","接管处(DW002)","总磷（以P计）","2025-11-12","","","","","0.08","1.5","","mg/L","否","","","是"]
["011","江苏华宜针织有限公司","水环境,大气环境","棉印染精加工","","纺织染整工业水污染物排放标准(GB4287-2012)","表2新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口","接管处(DW002)","化学需氧量","2025-11-12","","","","","112","200","","mg/L","否","","","是"]
["011","江苏华宜针织有限公司","水环境,大气环境","棉印染精加工","","纺织染整工业水污染物排放标准(GB4287-2012)","（表3）水污染物特别排放限值,企业废水总排放口,直接排放","接管处(DW002)","pH值","2025-11-12","","","","","8.2","9","6","无量纲","否","","","是"]